ADDENDUM #1

April 3, 2024

TO: Potential Offerors

FROM: Maia Guirao, Contract Manager

RE: Solicitation Addendum #1 to RFP #24-03/Raised Concrete Platform for

KVMH Install Walk-In Freezer

This correspondence serves as Addendum #1 to the subject Request for Proposals (“RFP”). Your response to this RFP should be governed by the content of the original RFP and the revisions/corrections/additions/clarifications provided in this addendum notice.

The following questions were asked:

1. Q: Pad was changed to 20’ wide to 25’, length of 45’ remains.

A: Yes.

1. Q: 4” thk SOG will have welded wire mesh, no rebar.

A: Yes.

1. Q: Frame wall height will be 9’ high.

A: Yes.

1. Q: Roof material will be peel and stick.

A: Yes.

1. Q: Siding T-1-11 (ruf sawn), no grooves.

A: Yes.

1. Q: Please advise if insulation if required in the walls & ceiling.  If yes, what kind?

A: No.

1. Q: Door will be 4’-0” x 6’-8”, solid wood door.

A: Yes.

1. Q: No permit required.

A: Correct, no permit is required.

1. Q: We will use concrete for retaining walls in lieu of CMU.

A: Okay to use concrete for retaining walls in lieu of CMU.